Lang{
"Anyka Burn Tool",
"Update Mode",
"File(&F)",
"Import File(&I)",
"Export File(&O)",
"Setting(&S)",
"Config Setting",
"Modify Password",
"View(&V)",
"Language",
"COM Window",
"Tool(&T)",
"Creat Spi Nor Flash Image Off Line(&I)",
"Upload Spi Nor Flash Image(&S)",
"Upload Bin(&B)",
"Config Files(&C)",
"Help(&H)",
"About Anyka Burn Tool(&A)",
"Start",
"Setting",
"Import",
"Export",
"Format",
"Status",
"Number",
"Progress",
"Status",
"Timer",
"Serial No.",
"Mac Addr",
"Device",
"Current Link:",
"Available Link:",
"Burn Count:",
"Total Pass:",
"Total Fail:",
"Clear",
"Burn State",
"USB Num:",
"Udisk:",
"Auto Burn",
"Udisk Burn",
"Online Make_Image(only device0 && make once)",
"No Fixed Channels",
"Udisk Massboot",
"Producer",
"Researcher",
"Input the User Name and Password:",
"User Name:",
"Password:",
"Change Password",
"User:",
"Old Password:",
"New Password:",
"Confirm Password:",
"Error Password!",
"Confirm Password Error!",
"Modify Password Success",
"Ready",
"Udisk update Ready",
"start burn",
"start to set RAM parameter",
"Fail to set RAM parameter",
"Begin to set registers",
"Fail to set registers",
"Fail to get registers",
"Set registers Sucessfully",
"Begin to init USB",
"Fail to init USB",
"Burn task complete",
"start test RAM",
"test RAM fail",
"Begin to download producer",
"Fail to download producer",
"Fail to connet usb after download producer",
"loading producer time out",
"Download producer Succcessfully",
"partition info is null",
"get medium data info fail",
"get free block info fail",
"Start to mount disk",
"Fail to mount disk",
"malloc medium fail",
"Start to Test",
"Fail to test",
"Begin to get nandflash chip id",
"Fail to get nandflash chip id",
"Begin to set nandflash chip parameter",
"Fail to set nandflash chip parameter",
"the spi parameter is not in spiflash list",
"set the ex parameter fail or set boot size error",
"Begin to get spiflash chip id",
"Fail to get spiflash chip id",
"Begin to set spiflash chip parameter",
"Fail to set spiflash chip parameter",
"Begin to erase",
"Fail to erase",
"Begin to format",
"Fail to format",
"Begin to download file",
"Fail to download file",
"Start to get activation file",
"Fail to get activation file",
"Project Name: ",
"Channel Number: ",
"Platform Type: ",
"Carrier burn, for no usb chip",
"Open COM",
"COM Number: ",
"COM Base: ",
"Baud Rate: ",
"Config Command Line",
"Addr:",
"Data:",
"Burn Mac Addr",
"Force Write Mac Addr",
"Current Mac Reset",
"Start Addr(0x):",
"End Addr(0x):",
"Burn Serial",
"Force Write Serial",
"Startprefix(0x):",
"Endprefix(0x):",
"Serial:",
"Burn Blue Addr",
"Force Write Blue Addr",
"Blue Start:",
"Blue End:",
"Browse",
"Producer: ",
"Boot: ",
"Boot(37L): ",
"Bios:",
"Burn Fs File",
"Burn Bin",
"Burn Fs Img",
"Burn Flash Img",
"No.",
"bCompare",
"YES",
"NO",
"PC Path",
"Download File",
"Download Directory",
"Udisk Path",
"Start Address",
"End Address",
"Backup Start Address",
"Backup End Address",
"Disk Name",
"Link Address",
"Part Name",
"bBackup",
"YES",
"NO",
"Bin Area Size(KB)",
"Chip Type: ",
"USB2.0",
"PLLFrep_change",
"Get Activation File",
"Update Mode",
"CPU_DDR2 FREQ",
"SET GPIO",
"FLASH",
"SYSTEM SETUP",
"Import...",
"Export...",
"Row:",
"Column:",
"USB Boot",
"Power Off GPIO",
"BIOS Start Address",
"FS Reserver Blocks",
"RAM Type: ",
"Size(M): ",
"Bank: ",
"Row Length: ",
"Col Address: ",
"ChipSel:",
"Manual",
"Chip0",
"Chip1",
"Chip2",
"Chip3",
"All",
"Init USB",
"Plug GPIO",
"Write Register",
"Register: ",
"Bit: ",
"Driver List: ",
"No.",
"Symbol",
"Type",
"Readonly",
"Hidden",
"Medium_type",
"Size(K)",
"Volume",
"FS Reserver Blocks",
"NonFS Reserve Size",
"Nandflash List: ",
"SpiNandflash List: ",
"Spiflash List:",
"Start Infineon module burn",
"Infineon module burn fail",
"device_synchronized!",
"failed to boot target board",
"Start to download fls file",
"Start to download eep file",
"failed to download fls file",
"failed to download eep file",
"download mode",
"AK only",
"Infineon only",
"Both",
"Burn Setting",
"Baudrate: ",
"download fls:",
"download eep:",
"Browse",
"GPIO Setting",
"GPIO Setting_fail",
"fail to set param to producer",
"start to download bin",
"fail to download bin",
"start to download img",
"fail to download img",
"format driver name and img driver name diffrent",
"start to download boot",
"fail to download boot",
"start write mac addr into asa",
"write mac addr into asa fail",
"start write serial addr into asa",
"write serial addr into asa fail",
"Begin to download change clk",
"Fail to download change clk",
"loading change clk time out",
"Fail to connet usb after download change clk",
"set burn mode",
"set burn mode fail",
"set burn erase mode",
"set burn erase mode fail",
"set nand para",
"set nand para fail",
"set security area",
"set security area fail",
"bin upload fail",
"get bad block information fail",
"read mac addr in asafile",
"read mac addr  error",
"read serial addr in asafile",
"read serial addr error",
"burn mac addr compare",
"burn mac addr beyond the most",
"burn serial addr compare",
"burn serial addr beyond the most",
"set reserve area",
"set reserve area fail",
"create partition",
"create partition fail",
"close",
"close fail",
"pls input the num must be 0~9，A~F，a~f",
"MAC Addr format must be 00:00:00",
"mac start addr high Length less than 8 !!",
"mac start addr low Length less than 8 !!",
"mac end addr high Length less than 8 !!",
"mac end addr low Length less than 8 !!",
"the string is not 0~9，A~F，a~f !!!!",
"h_mac_start_addr and h_end_addr is differnt!!",
"l_mac_start addr is more than l_mac_end_addr !!",
"h_serial_start_addr str Length less than 10 !!",
"l_serial_start_addr str Length less than 6 !!",
"h_serial_end_addr str Length less than 10 !!",
"l_serial_end_addr str Length less than 6 !!",
"h_serial_start_addr and h_end_addr is differnt!!",
"l_serial_start_addr is more than l_end_addr!!",
"mac addr  reset succeed, current = start !!",
"current serial  reset succeed, current = start !!",
"start set channel id",
"get the channel id is error",
"Image Create Box",
"sourcefolder:",
"destfolder:",
"Browse",
"Browse",
"Imagename:",
"capacity(MByte):",
"pagesize(Byte):",
"sectorsize(Byte):",
"make information:",
"Ready Image make...",
"Image making...",
"Begin",
"End",
"Image make success!!",
"Image make fail!!",
"getting folder info!!",
"get folder info fail!!",
"capacity size is no enough!!",
"param error!!",
"source folder empty!",
"Destination folder empty!",
"image name empty!",
"capacity empty!",
"sector empty!",
"page size empty!",
"set nand gpioce fail!",
"download channel addr fail!",
"set com mode fail!",
"download com mode fail!",
"image making",
"make image success!",
"make image fail!",
"finish make image and reset!",
"Process is running, make sure to close or no!",
"Enter the verification string",
"Import file success!",
"Import file fail!",
"wait...",
"Export file success!",
"Export file fail!",
"All data will be lost, make sure to format or not",
"Spi Nor Flash Mirror",
"Choose the flash, please!",
"SPI:",
"No SPI can choose",
"Open help file error",
"Physical Format",
"OK",
"Cancel",
"driver volume name must not be",
"the mac addr is special addr，please modification",
"the mac addr can not be zero",
"get highID fail,produce is not too old",
"before creat disk to get all free block",
"the capacity of the nand/sd is differnt",
"check the capacity of ervery device",
"Bin upload complete",
"Bin upload, please enter massboot to start",
"Spi flash upload complete",
"Spi flash upload fail",
"Spi flash upload, please enter massboot to start",
"start upload spiflash all data",
"read OTP serial",
"read OTP serial fail",
"write OTP serial",
"write OTP serial fail",
"OTP serial is existed",
"no find bin name in partition",
"get partiton size error",
"start burn ENV",
"burn ENV FAIL",
"partition name and bin name diffrent",
"download spiflash img fail",
"SPI img file only one",
"download spiflash img start",
"download spiflash img finish",
"Erase For Start Burn(erase all partition size,erase size is 64K)",
"No Need Erase For Burn(the spiflash is new,no need erase)",
"name len more than 8",
"start erase partition",
"erase partition fail",
"check fs type fail",
"get blue addr start",
"blue addr more than end addr",
"blue addr len error",
"blue addr error",
"write blue addr fail",
"start write blue addr",
"erase block more than total num",
"erase block 0 ",
"erase block 0 fail",
"set kernel pos flag",
"kernel pos(K):",
"jiggle mode(no vin_chg)",
"Check_Info",
"Create UBoot(&U)",
"Uboot Mirror",
"Choose the flash, please!",
"Offset(0x)",
"Size(0x)",
"Erase All Partition",
"Update",
}
